|  |  |
| --- | --- |
|  | Additional Information |

This notice includes information related to your product. Please read this sheet carefully and retain for your reference.

1. Jumper Settings

**1.1 In normal use, the V9958 video board requires a jumper between pins 9 and 11 of J2.**

The included pin header for J2 has this jumper pre-installed for you.

This jumper is not required if external hardware is being used to provide video sync information.

In cases where a daughterboard is being connected to J2 and external sync is not being used, this connection should be made on the daughterboard (or, for example, a jumper may be provided for this purpose).

**1.2 JP1 Jumper for revision 1.2 main board**

If you have a revision 1.2 main board, you will need to connect a jumper to JP1 to enable DTACK handling. A header and jumper is included in pack 3 for this.

**If you have a revision 1 board, do not connect this jumper. Although unlikely, it is possible damage may occur if this jumper is connected when used with a revision 1 board.**